(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "Green") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (color "Green") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (aux_axis_origin 108.585 121.92)
    (grid_origin 108.585 121.92)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0001000_00000000)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes false)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 6)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "/media/dd_1To/PERSO_2/ELECTRON/ESP/CARTE_ESP32_TFT/Kicad/CARTE_ESP32_TFT/GERBER/")
    )
  )
  (net 0 "")
  (net 1 "Net-(P1-Pad1)")
  (net 2 "Net-(R1-Pad1)")
  (net 3 "Net-(P2-Pad1)")
  (net 4 "unconnected-(U1-Pad1)")
  (net 5 "unconnected-(U1-Pad2)")
  (net 6 "Net-(P3-Pad1)")
  (net 7 "Net-(U1-Pad22)")
  (net 8 "unconnected-(U1-Pad4)")
  (net 9 "Net-(U1-Pad10)")
  (net 10 "Net-(U1-Pad9)")
  (net 11 "Net-(U1-Pad11)")
  (net 12 "unconnected-(U1-Pad6)")
  (net 13 "Net-(U1-Pad21)")
  (net 14 "Net-(U1-Pad8)")
  (net 15 "unconnected-(U1-Pad12)")
  (net 16 "unconnected-(U1-Pad13)")
  (net 17 "unconnected-(U1-Pad14)")
  (net 18 "Net-(U1-Pad3)")
  (net 19 "Net-(U1-Pad15)")
  (net 20 "Net-(U1-Pad16)")
  (net 21 "Net-(U1-Pad17)")
  (net 22 "Net-(U1-Pad18)")
  (net 23 "GND")
  (net 24 "Net-(U1-Pad19)")
  (net 25 "Net-(U1-Pad20)")
  (net 26 "Net-(P4-Pad1)")
  (net 27 "Net-(U1-Pad7)")
  (net 28 "Net-(U1-Pad23)")
  (net 29 "Net-(U1-Pad24)")
  (net 30 "unconnected-(U1-Pad27)")
  (net 31 "unconnected-(U1-Pad28)")
  (net 32 "Net-(U1-Pad25)")
  (net 33 "Net-(U1-Pad26)")
  (net 34 "unconnected-(U2-Pad12)")
  (net 35 "unconnected-(U2-Pad16)")
  (net 36 "Net-(P5-Pad1)")
  (net 37 "Net-(P6-Pad1)")
  (net 38 "unconnected-(U2-Pad13)")
  (footprint "Resistor_perso:R_300" (layer "F.Cu")
    (at 147.955 92.71 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "CARTE_ESP32_TFT.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R4" (at 3.937 0 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 4.064 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.8 1.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 26 "Net-(P4-Pad1)"))
    (pad "2" thru_hole circle (at 7.62 0 90) (size 1.8 1.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(R1-Pad1)"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connect_perso:E-S_3mm" (layer "F.Cu")
    (at 163.195 100.33)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags "DEV")
    (property "Sheetfile" "CARTE_ESP32_TFT.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P3" (at 2.54 0) (layer "F.SilkS"))
    (fp_text value "P" (at -3.048 1.016) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.5) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 6 "Net-(P3-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "TFT:TFT_Shield_480x320" (layer "F.Cu")
    (at 122.555 118.11)
    (property "Sheetfile" "CARTE_ESP32_TFT.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "U1" (at -1.27 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "TFT_480x320" (at 0 -19.05 unlocked) (layer "F.Fab"))
    (fp_text user "3.5\" TFT LCD Shield" (at 6.35 -35.56 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at -3.81 -3.81 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -2.54 0) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "unconnected-(U1-Pad1)"))
    (pad "2" thru_hole circle (at 0 0) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 5 "unconnected-(U1-Pad2)") (pinfunction "3V3"))
    (pad "3" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 18 "Net-(U1-Pad3)") (pinfunction "5V"))
    (pad "4" thru_hole circle (at 5.08 0) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "unconnected-(U1-Pad4)"))
    (pad "5" thru_hole circle (at 7.62 0) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 23 "GND") (pinfunction "GND"))
    (pad "6" thru_hole circle (at 10.16 0) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 12 "unconnected-(U1-Pad6)"))
    (pad "7" thru_hole circle (at 15.24 0) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 27 "Net-(U1-Pad7)") (pinfunction "LCD_RD"))
    (pad "8" thru_hole circle (at 17.78 0) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(U1-Pad8)") (pinfunction "LCD_WR"))
    (pad "9" thru_hole circle (at 20.32 0) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(U1-Pad9)") (pinfunction "LCD_RS"))
    (pad "10" thru_hole circle (at 22.86 0) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(U1-Pad10)") (pinfunction "LCD_CS"))
    (pad "11" thru_hole circle (at 25.4 0) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(U1-Pad11)") (pinfunction "LCD_RST"))
    (pad "12" thru_hole circle (at 27.94 0) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 15 "unconnected-(U1-Pad12)"))
    (pad "13" thru_hole circle (at 27.94 -48.26) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "unconnected-(U1-Pad13)"))
    (pad "14" thru_hole circle (at 25.4 -48.26) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 17 "unconnected-(U1-Pad14)"))
    (pad "15" thru_hole circle (at 22.86 -48.26) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(U1-Pad15)") (pinfunction "LCD_02"))
    (pad "16" thru_hole circle (at 20.32 -48.26) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(U1-Pad16)") (pinfunction "LCD_03"))
    (pad "17" thru_hole circle (at 17.78 -48.26) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 21 "Net-(U1-Pad17)") (pinfunction "LCD_04"))
    (pad "18" thru_hole circle (at 15.24 -48.26) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 22 "Net-(U1-Pad18)") (pinfunction "LCD_05"))
    (pad "19" thru_hole circle (at 12.7 -48.26) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 24 "Net-(U1-Pad19)") (pinfunction "LCD_06"))
    (pad "20" thru_hole circle (at 10.16 -48.26) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 25 "Net-(U1-Pad20)") (pinfunction "LCD_07"))
    (pad "21" thru_hole circle (at 6.35 -48.26) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(U1-Pad21)") (pinfunction "LCD_00"))
    (pad "22" thru_hole circle (at 3.81 -48.26) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(U1-Pad22)") (pinfunction "LCD_01"))
    (pad "23" thru_hole circle (at 1.27 -48.26) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 28 "Net-(U1-Pad23)") (pinfunction "SD_SS"))
    (pad "24" thru_hole circle (at -1.27 -48.26) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(U1-Pad24)") (pinfunction "SD_DI"))
    (pad "25" thru_hole circle (at -3.81 -48.26) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 32 "Net-(U1-Pad25)") (pinfunction "SD_DO"))
    (pad "26" thru_hole circle (at -6.35 -48.26) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 33 "Net-(U1-Pad26)") (pinfunction "SD_SCK"))
    (pad "27" thru_hole circle (at -8.89 -48.26) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 30 "unconnected-(U1-Pad27)"))
    (pad "28" thru_hole circle (at -11.43 -48.26) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 31 "unconnected-(U1-Pad28)"))
  )
  (footprint "Connect_perso:E-S_3mm" (layer "F.Cu")
    (at 163.195 97.79)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags "DEV")
    (property "Sheetfile" "CARTE_ESP32_TFT.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P4" (at 2.54 0) (layer "F.SilkS"))
    (fp_text value "P" (at -3.048 1.016) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.5) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 26 "Net-(P4-Pad1)") (pinfunction "1"))
  )
  (footprint "Connect_perso:E-S_3mm" (layer "F.Cu")
    (at 163.195 110.49)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags "DEV")
    (property "Sheetfile" "CARTE_ESP32_TFT.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P7" (at 2.54 0) (layer "F.SilkS"))
    (fp_text value "P" (at -3.048 1.016) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.5) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 23 "GND") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Connect_perso:E-S_3mm" (layer "F.Cu")
    (at 163.195 105.41)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags "DEV")
    (property "Sheetfile" "CARTE_ESP32_TFT.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P2" (at 2.54 0) (layer "F.SilkS"))
    (fp_text value "P" (at -3.048 1.016) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.5) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 3 "Net-(P2-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_perso:R_300" (layer "F.Cu")
    (at 151.765 92.71 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "CARTE_ESP32_TFT.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R3" (at 3.937 0 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 4.064 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.8 1.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(P3-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 7.62 0 90) (size 1.8 1.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(R1-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connect_perso:E-S_3mm" (layer "F.Cu")
    (at 163.195 107.95)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags "DEV")
    (property "Sheetfile" "CARTE_ESP32_TFT.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P1" (at 2.54 0) (layer "F.SilkS"))
    (fp_text value "P" (at -3.048 1.016) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.5) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 1 "Net-(P1-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Connect_perso:E-S_3mm" (layer "F.Cu")
    (at 163.195 102.87)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags "DEV")
    (property "Sheetfile" "CARTE_ESP32_TFT.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P5" (at 2.54 0) (layer "F.SilkS"))
    (fp_text value "P" (at -3.048 1.016) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.5) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 36 "Net-(P5-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_perso:R_300" (layer "F.Cu")
    (at 140.335 85.09 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "CARTE_ESP32_TFT.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R1" (at 3.937 0 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 4.064 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.8 1.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(R1-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 7.62 0 270) (size 1.8 1.8) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 37 "Net-(P6-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connect_perso:E-S_3mm" (layer "F.Cu")
    (at 163.195 95.25)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags "DEV")
    (property "Sheetfile" "CARTE_ESP32_TFT.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P6" (at 2.54 0) (layer "F.SilkS"))
    (fp_text value "P" (at -3.048 1.016) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.5) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 37 "Net-(P6-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "ESP32:ESP32_30pins" (layer "B.Cu")
    (at 116.205 79.375)
    (property "Sheetfile" "CARTE_ESP32_TFT.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at 7.62 21.59 180 unlocked) (layer "B.SilkS"))
    (fp_text value "ESP32_30pins" (at 6.35 19.05 180 unlocked) (layer "B.Fab"))
    (fp_text user "( module cote composants )" (at 24.13 22.86 180 unlocked) (layer "B.SilkS"))
    (fp_text user "( cote composants )" (at 6.35 11.43 180 unlocked) (layer "B.SilkS"))
    (fp_text user "ESP-WROOM-32" (at 6.35 14.605 180 unlocked) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 7.62 16.51 180 unlocked) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(R1-Pad1)") (pinfunction "3V3") (pintype "input"))
    (pad "2" thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 23 "GND") (pinfunction "GND") (pintype "input"))
    (pad "3" thru_hole circle (at 5.08 0 180) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 22 "Net-(U1-Pad18)") (pinfunction "15") (pintype "input"))
    (pad "4" thru_hole circle (at 7.62 0 180) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(U1-Pad15)") (pinfunction "2") (pintype "input"))
    (pad "5" thru_hole circle (at 10.16 0 180) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(U1-Pad22)") (pinfunction "4") (pintype "input"))
    (pad "6" thru_hole circle (at 12.7 0 180) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(U1-Pad21)") (pinfunction "16") (pintype "input"))
    (pad "7" thru_hole circle (at 15.24 0 180) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 25 "Net-(U1-Pad20)") (pinfunction "17") (pintype "input"))
    (pad "8" thru_hole circle (at 17.78 0 180) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 28 "Net-(U1-Pad23)") (pinfunction "5") (pintype "input"))
    (pad "9" thru_hole circle (at 20.32 0 180) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 33 "Net-(U1-Pad26)") (pinfunction "18_SCK") (pintype "input"))
    (pad "10" thru_hole circle (at 22.86 0 180) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 32 "Net-(U1-Pad25)") (pinfunction "19_MISO") (pintype "input"))
    (pad "11" thru_hole circle (at 25.4 0 180) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 21 "Net-(U1-Pad17)") (pinfunction "21") (pintype "input"))
    (pad "12" thru_hole circle (at 27.94 0 180) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 34 "unconnected-(U2-Pad12)") (pinfunction "3") (pintype "input"))
    (pad "13" thru_hole circle (at 30.48 0 180) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 38 "unconnected-(U2-Pad13)") (pinfunction "1") (pintype "input"))
    (pad "14" thru_hole circle (at 33.02 0 180) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(U1-Pad16)") (pinfunction "22") (pintype "input"))
    (pad "15" thru_hole circle (at 35.56 0 180) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(U1-Pad24)") (pinfunction "23_MOSI") (pintype "input"))
    (pad "16" thru_hole circle (at 35.56 25.4 180) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 35 "unconnected-(U2-Pad16)") (pinfunction "EN") (pintype "input"))
    (pad "17" thru_hole circle (at 33.02 25.4 180) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(P3-Pad1)") (pinfunction "36") (pintype "input"))
    (pad "18" thru_hole circle (at 30.48 25.4 180) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 26 "Net-(P4-Pad1)") (pinfunction "39") (pintype "input"))
    (pad "19" thru_hole circle (at 27.94 25.4 180) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 36 "Net-(P5-Pad1)") (pinfunction "34") (pintype "input"))
    (pad "20" thru_hole circle (at 25.4 25.4 180) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 37 "Net-(P6-Pad1)") (pinfunction "35") (pintype "input"))
    (pad "21" thru_hole circle (at 22.86 25.4 180) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(P2-Pad1)") (pinfunction "32") (pintype "input"))
    (pad "22" thru_hole circle (at 20.32 25.4 180) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(P1-Pad1)") (pinfunction "33") (pintype "input"))
    (pad "23" thru_hole circle (at 17.78 25.4 180) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 24 "Net-(U1-Pad19)") (pinfunction "25") (pintype "input"))
    (pad "24" thru_hole circle (at 15.24 25.4 180) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(U1-Pad11)") (pinfunction "26") (pintype "input"))
    (pad "25" thru_hole circle (at 12.7 25.4 180) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(U1-Pad10)") (pinfunction "27") (pintype "input"))
    (pad "26" thru_hole circle (at 10.16 25.4 180) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(U1-Pad9)") (pinfunction "14") (pintype "input"))
    (pad "27" thru_hole circle (at 7.62 25.4 180) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(U1-Pad8)") (pinfunction "12") (pintype "input"))
    (pad "28" thru_hole circle (at 5.08 25.4 180) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 27 "Net-(U1-Pad7)") (pinfunction "13") (pintype "input"))
    (pad "29" thru_hole circle (at 2.54 25.4 180) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 23 "GND") (pinfunction "GND") (pintype "input"))
    (pad "30" thru_hole circle (at 0 25.4 180) (size 1.8 1.8) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 18 "Net-(U1-Pad3)") (pinfunction "VIN") (pintype "input"))
  )
  (gr_rect (start 108.585 64.77) (end 167.005 121.92)
    (fill none) (layer "Edge.Cuts"))
)
